The ZIP file “Tri-Flex Loop” contains the catalog standards of the Tri-Flex Loop™ for both +/- 2” of motion and +/- 4” of motion, ˝”ID – 12” ID nominal sizes.  The included styles are:
FHTFL2/4SMN Stainless steel hose & braid with carbon steel male NPT each end.
FHTFL2/4SMP Stainless steel hose & braid with 150# carbon steel plate flanges each end.
FHTFL2/4SVG Stainless steel hose & braid with carbon steel grooved pipe ends.
FHTFL2/4SWN Stainless steel hose & braid with beveled carbon steel weld ends.
FHTFL2/4BSW Bronze hose & braid with copper female sweat ends.
FHTFL2/4BPP Bronze hose & braid with copper female press fit ends.
The UL-536 listed loops for compressed and flammable gases are also included for sizes 1”-4” ID in the threaded, flanged and weld end styles.

Note: In each case there is a file with and without an interference box. The interference box is meant to show the potential footprint of the loop when fully compressed, extended or offset.

